\index{instructions}
\begin{figure}[hbt]
\centering
\includegraphics[keepaspectratio=true,angle=0,height=0.4\textheight,width=1.0\textwidth]{shipping_clamps.jpg}
\caption{Red Shipping Clamps}
\label{fig:shipping_clamps}
\end{figure}
\begin{enumerate}
\item Remove the plastic bag containing instructions, cords, and small parts.

\index{foam padding}
\item Remove the top foam padding. 

\index{filament spool}
\item Slowly remove the two smaller foam pads. One of these pads will contain the plastic filament spool.

\index{power supply}
\item Remove the bubble wrapped power supply.

\item Grab the top of the wrapped printer on the top center where you will feel two lengths of square aluminum tubing. Holding the top two tubes, SLOWLY pull the printer upwards out of the box. The two large side foam pads should fall off when the printer is out of the box.

\item Set you printer on a stable level surface.

\item Gently unwrap the pink ESD plastic covering the printer. Gently lift the printer to slide the plastic wrapping from under the printer. 

\item Using scissors or wire cutters, cut and remove the two ORANGE plastic zip ties
(Fig. \ref{fig:zip_ties}, page \pageref{fig:zip_ties})
. One zip tie is located on the bottom front of the printer on the print bed. The other zip tie is around the extruder carriage and X axis. Make sure to not cut any of the surrounding wires or belts.

\begin{figure}[hbt]
\centering
\includegraphics[keepaspectratio=true,angle=0,height=0.4\textheight,width=1.0\textwidth]{zip_ties.jpg}
\caption{Orange Zip Ties}
\label{fig:zip_ties}
\end{figure}

\item Find the item list attached to the plastic bag of parts. Before you move on to setting up your printer make sure all of the items on the list are in your package.

\index{shipping clamps}
\index{x-end motor mount}
\index{idler}
\item Remove the four red shipping clamps above and below the x-end motor mount and idler
(Fig. \ref{fig:shipping_clamps}, page \pageref{fig:shipping_clamps}).

Loosen and remove the wing nut and screw on each of the four clamps. Remove each of the four clamps by popping them off of the smooth rod. Keep the clamps and hardware for future use if you need to ship or transport your printer.

\index{blue tape}
\index{PET tape}
\item Remove the blue tape from two sides of the print surface. Make sure to not remove the green PET tape on the glass print surface. The PET tape helps keep the print attached to the print surface during printing.

\end{enumerate}
