(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 49)
    (no_connects 0)
    (area 50.854 77.39954 111.706001 116.85582)
    (thickness 1.6)
    (drawings 9)
    (tracks 138)
    (zones 0)
    (modules 26)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.016)
    (via_drill 0.508)
    (via_min_size 1.016)
    (via_min_drill 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Z_Brake_Gerbers_Rev_B/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 GND)
  (net 5 +24V)
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(K1-Pad10)")
  (net 9 "Net-(K1-Pad9)")
  (net 10 "Net-(K1-Pad8)")
  (net 11 "Net-(K1-Pad4)")
  (net 12 "Net-(K1-Pad5)")
  (net 13 "Net-(K2-Pad10)")
  (net 14 "Net-(K2-Pad9)")
  (net 15 "Net-(K2-Pad8)")
  (net 16 "Net-(K2-Pad4)")
  (net 17 "Net-(K2-Pad5)")
  (net 18 "Net-(Q1-Pad1)")
  (net 19 VDD)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(K1-Pad10)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K1-Pad5)")
    (add_net "Net-(K1-Pad8)")
    (add_net "Net-(K1-Pad9)")
    (add_net "Net-(K2-Pad10)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(K2-Pad5)")
    (add_net "Net-(K2-Pad8)")
    (add_net "Net-(K2-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net VDD)
  )
  (net_class STD_Signal ""
    (clearance 0.2)
    (trace_width 0.3048)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module "AO Parts:EC2_Relay" (layer F.Cu) (tedit 5A60B19A)
    (at 93.98 96.52 90)
    (fp_text reference K1 (at 7.2 -5 180) (layer F.SilkS))
    (fp_text value EC2-24NU (at 0 -5.08 90) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(K1-Pad10)"))
    (pad 9 thru_hole circle (at 2.54 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(K1-Pad9)"))
    (pad 8 thru_hole circle (at 5.08 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(K1-Pad8)"))
    (pad 12 thru_hole circle (at -5.08 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 VDD))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(K1-Pad10)"))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(K1-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(K1-Pad5)"))
  )
  (module "AO Parts:EC2_Relay" (layer F.Cu) (tedit 5A60B129)
    (at 81.28 96.52 90)
    (fp_text reference K2 (at 7.2 5.2 180) (layer F.SilkS))
    (fp_text value EC2-24NU (at 0 -5.08 90) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(K2-Pad10)"))
    (pad 9 thru_hole circle (at 2.54 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(K2-Pad9)"))
    (pad 8 thru_hole circle (at 5.08 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(K2-Pad8)"))
    (pad 12 thru_hole circle (at -5.08 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at -5.08 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 VDD))
    (pad 3 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(K2-Pad10)"))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(K2-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(K2-Pad5)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A298C4E)
    (at 68.58 102.87 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Handsoldering (layer F.Cu) (tedit 5A299AE6)
    (at 66.675 89.535)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 -2.85) (layer F.SilkS))
    (fp_text value "10.0 V ZENER" (at 0.05 4.4) (layer F.Fab) hide)
    (fp_text user A (at 5.08 0) (layer F.SilkS))
    (fp_text user K (at -5.08 0) (layer F.SilkS))
    (pad 1 smd rect (at -2.49936 0) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.49936 0) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Diodes_SMD.3dshapes/SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5A286E24)
    (at 93.98 104.775 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -2 180) (layer F.SilkS))
    (fp_text value D_Schottky_ALT (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5A286E2D)
    (at 81.28 104.775 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 -2 180) (layer F.SilkS))
    (fp_text value D_Schottky_ALT (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A2984E8)
    (at 74.676 90.678)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.9) (layer F.SilkS))
    (fp_text value LED_ALT (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A299DF1)
    (at 73.66 101.6 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 3.175 0 360) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A299DE1)
    (at 60.96 96.52 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -3.175 0 360) (layer F.SilkS))
    (fp_text value 12.6k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A299DEA)
    (at 62.865 101.6 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A299DDE)
    (at 63.5 96.52 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.175 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A298C4B)
    (at 68.58 105.41 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A6107E6)
    (at 68.58 93.98)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A6107EA)
    (at 72.39 95.25 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.794 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A29898C)
    (at 74.676 95.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 3.3k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A298BA5)
    (at 68.58 99.06)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -0.05 -2.55) (layer F.SilkS))
    (fp_text value LM397 (at -0.05 2.35) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A2984E0)
    (at 91.44 83.82 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 10.668 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(K1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(K1-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(K2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(K2-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5A298999)
    (at 68.58 83.82 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -3.175 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +24V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A2984BB)
    (at 97.79 109.22 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -2.54 -1.27 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(K1-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(K1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(K2-Pad4)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(K2-Pad10)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5A2984C4)
    (at 85.09 109.22 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -2.54 8.89 360) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(K1-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(K1-Pad9)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(K2-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(K2-Pad9)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "AO Parts:MOUNT_HOLE" (layer F.Cu) (tedit 55116EF0)
    (at 58.42 83.82)
    (fp_text reference MH1 (at 0 -5.00126) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.096 6.096) (drill 3.175) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module "AO Parts:MOUNT_HOLE" (layer F.Cu) (tedit 55116EF0)
    (at 104.14 83.82)
    (fp_text reference MH2 (at 0 -5.00126) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.096 6.096) (drill 3.175) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module "AO Parts:MOUNT_HOLE" (layer F.Cu) (tedit 55116EF0)
    (at 58.42 109.22)
    (fp_text reference MH3 (at 0 -5.00126) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.096 6.096) (drill 3.175) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module "AO Parts:MOUNT_HOLE" (layer F.Cu) (tedit 55116EF0)
    (at 104.14 109.22)
    (fp_text reference MH4 (at 0 -5.00126) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.096 6.096) (drill 3.175) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5A29A339)
    (at 68.58 109.22)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab) hide)
  )
  (module Diodes_SMD:SMA_Handsoldering (layer F.Cu) (tedit 5A6108A5)
    (at 74.676 84.582 90)
    (descr "Diode SMA Handsoldering")
    (tags "Diode SMA Handsoldering")
    (attr smd)
    (fp_text reference D5 (at 0 3.048 180) (layer F.SilkS))
    (fp_text value D_ALT (at 0.05 4.4 90) (layer F.Fab) hide)
    (fp_text user A (at 3.05 2.85 90) (layer F.SilkS))
    (fp_text user K (at -3.25 2.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.49936 0 90) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 2.49936 0 90) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 +24V))
    (model Diodes_SMD.3dshapes/SMA_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text PC-BD0096 (at 87.63 112.268) (layer F.SilkS))
  (gr_text "REV. B" (at 104.8258 98.2218 90) (layer F.SilkS))
  (gr_text GPLv3 (at 95.7834 83.9978 90) (layer F.SilkS))
  (gr_text "© 2018 Aleph Objects" (at 99.2632 92.456 90) (layer F.SilkS))
  (gr_text "Motor Brake" (at 102.0318 95.0976 90) (layer F.SilkS))
  (gr_line (start 53.34 114.3) (end 53.34 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 114.3) (end 53.34 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 78.74) (end 109.22 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 78.74) (end 109.22 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 108.585 113.665) (xy 53.975 113.665) (xy 53.975 79.375) (xy 108.585 79.375)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 108.585 113.665) (xy 53.975 113.665) (xy 53.975 79.375) (xy 108.585 79.375)
      )
    )
  )
)
