(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 281)
    (no_connects 3)
    (area 67.899999 45.899999 202.888096 134.100001)
    (thickness 1.6)
    (drawings 20)
    (tracks 1427)
    (zones 0)
    (modules 82)
    (nets 106)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.4 2.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e8_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers_Rev_A/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(C12-Pad1)")
  (net 6 "Net-(CP3-Pad8)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(LS1-Pad2)")
  (net 11 "Net-(P1-Pad5)")
  (net 12 "Net-(RN3-Pad8)")
  (net 13 "Net-(RN3-Pad9)")
  (net 14 /B2)
  (net 15 /B3)
  (net 16 /B4)
  (net 17 /B5)
  (net 18 /B6)
  (net 19 /B7)
  (net 20 /F_R2)
  (net 21 /F_R3)
  (net 22 /F_R4)
  (net 23 /F_R5)
  (net 24 /F_R6)
  (net 25 /F_R7)
  (net 26 /F_G2)
  (net 27 /F_G3)
  (net 28 /F_G4)
  (net 29 /F_G5)
  (net 30 /F_G6)
  (net 31 /F_G7)
  (net 32 /F_B2)
  (net 33 /F_B3)
  (net 34 /F_B4)
  (net 35 /F_B5)
  (net 36 /F_B6)
  (net 37 /F_B7)
  (net 38 /F_PCLK)
  (net 39 /F_DISP)
  (net 40 /F_HSYNC)
  (net 41 /F_VSYNC)
  (net 42 /F_DE)
  (net 43 /XP)
  (net 44 /YM)
  (net 45 /XM)
  (net 46 /YP)
  (net 47 /R2)
  (net 48 /R3)
  (net 49 /R4)
  (net 50 /R5)
  (net 51 /R6)
  (net 52 /R7)
  (net 53 /G2)
  (net 54 /G3)
  (net 55 /G4)
  (net 56 /G5)
  (net 57 /G6)
  (net 58 /G7)
  (net 59 /PCLK)
  (net 60 /DISP)
  (net 61 /HSYNC)
  (net 62 /VSYNC)
  (net 63 /DE)
  (net 64 "Net-(P1-Pad4)")
  (net 65 "Net-(C1-Pad1)")
  (net 66 "Net-(C13-Pad1)")
  (net 67 "Net-(P1-Pad3)")
  (net 68 "Net-(P1-Pad9)")
  (net 69 "Net-(P1-Pad8)")
  (net 70 "Net-(P1-Pad6)")
  (net 71 "Net-(R11-Pad1)")
  (net 72 "Net-(R12-Pad1)")
  (net 73 "Net-(R13-Pad1)")
  (net 74 "Net-(R14-Pad1)")
  (net 75 "Net-(U1-Pad12)")
  (net 76 "Net-(U1-Pad10)")
  (net 77 "Net-(U1-Pad6)")
  (net 78 "Net-(U1-Pad4)")
  (net 79 "Net-(U1-Pad2)")
  (net 80 "Net-(U1-Pad15)")
  (net 81 "Net-(U3-Pad13)")
  (net 82 "Net-(U3-Pad14)")
  (net 83 "Net-(U3-Pad24)")
  (net 84 "Net-(U3-Pad7)")
  (net 85 "Net-(U3-Pad8)")
  (net 86 "Net-(U3-Pad10)")
  (net 87 "Net-(C8-Pad1)")
  (net 88 "Net-(C10-Pad1)")
  (net 89 "Net-(C14-Pad1)")
  (net 90 "Net-(C18-Pad1)")
  (net 91 "Net-(P1-Pad7)")
  (net 92 "Net-(P3-Pad8)")
  (net 93 "Net-(P3-Pad9)")
  (net 94 "Net-(P3-Pad10)")
  (net 95 "Net-(P4-Pad1)")
  (net 96 "Net-(P4-Pad13)")
  (net 97 "Net-(P4-Pad14)")
  (net 98 "Net-(P4-Pad35)")
  (net 99 "Net-(P5-Pad35)")
  (net 100 "Net-(R15-Pad1)")
  (net 101 "Net-(R16-Pad1)")
  (net 102 "Net-(R17-Pad1)")
  (net 103 "Net-(R18-Pad2)")
  (net 104 "Net-(LS1-Pad1)")
  (net 105 "Net-(R21-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /B2)
    (add_net /B3)
    (add_net /B4)
    (add_net /B5)
    (add_net /B6)
    (add_net /B7)
    (add_net /DE)
    (add_net /DISP)
    (add_net /F_B2)
    (add_net /F_B3)
    (add_net /F_B4)
    (add_net /F_B5)
    (add_net /F_B6)
    (add_net /F_B7)
    (add_net /F_DE)
    (add_net /F_DISP)
    (add_net /F_G2)
    (add_net /F_G3)
    (add_net /F_G4)
    (add_net /F_G5)
    (add_net /F_G6)
    (add_net /F_G7)
    (add_net /F_HSYNC)
    (add_net /F_PCLK)
    (add_net /F_R2)
    (add_net /F_R3)
    (add_net /F_R4)
    (add_net /F_R5)
    (add_net /F_R6)
    (add_net /F_R7)
    (add_net /F_VSYNC)
    (add_net /G2)
    (add_net /G3)
    (add_net /G4)
    (add_net /G5)
    (add_net /G6)
    (add_net /G7)
    (add_net /HSYNC)
    (add_net /PCLK)
    (add_net /R2)
    (add_net /R3)
    (add_net /R4)
    (add_net /R5)
    (add_net /R6)
    (add_net /R7)
    (add_net /VSYNC)
    (add_net /XM)
    (add_net /XP)
    (add_net /YM)
    (add_net /YP)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(CP3-Pad8)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(LS1-Pad1)")
    (add_net "Net-(LS1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(P3-Pad9)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad13)")
    (add_net "Net-(P4-Pad14)")
    (add_net "Net-(P4-Pad35)")
    (add_net "Net-(P5-Pad35)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(RN3-Pad8)")
    (add_net "Net-(RN3-Pad9)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad24)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
  )
  (net_class PWR ""
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5B07329F)
    (at 123.5 58.75)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at -0.25 3.25 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.09906 3.59918) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:IDC_Header_Straight_10pins (layer F.Cu) (tedit 5AFF49D5)
    (at 79 80 90)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P1 (at 16.5 -4.5 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 5.08 5.223 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C1-Pad1)"))
  )
  (module AO_Parts:FPC_40 (layer F.Cu) (tedit 5B059BEB)
    (at 154.75 83.5 180)
    (attr smd)
    (fp_text reference P4 (at -14 -6.25 180) (layer F.SilkS))
    (fp_text value FPC_40 (at 0 -3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -9.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at -9.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C18-Pad1)"))
    (pad 3 smd rect (at -8.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -8.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -7.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 6 smd rect (at -7.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 7 smd rect (at -6.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /F_R2))
    (pad 8 smd rect (at -6.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /F_R3))
    (pad 9 smd rect (at -5.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /F_R4))
    (pad 10 smd rect (at -5.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /F_R5))
    (pad 11 smd rect (at -4.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /F_R6))
    (pad 12 smd rect (at -4.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /F_R7))
    (pad 13 smd rect (at -3.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 14 smd rect (at -3.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 15 smd rect (at -2.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /F_G2))
    (pad 16 smd rect (at -2.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /F_G3))
    (pad 17 smd rect (at -1.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /F_G4))
    (pad 18 smd rect (at -1.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /F_G5))
    (pad 19 smd rect (at -0.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /F_G6))
    (pad 20 smd rect (at -0.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /F_G7))
    (pad 21 smd rect (at 0.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 22 smd rect (at 0.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 23 smd rect (at 1.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /F_B2))
    (pad 24 smd rect (at 1.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /F_B3))
    (pad 25 smd rect (at 2.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /F_B4))
    (pad 26 smd rect (at 2.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /F_B5))
    (pad 27 smd rect (at 3.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /F_B6))
    (pad 28 smd rect (at 3.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /F_B7))
    (pad 29 smd rect (at 4.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at 4.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /F_PCLK))
    (pad 31 smd rect (at 5.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 /F_DISP))
    (pad 32 smd rect (at 5.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 /F_HSYNC))
    (pad 33 smd rect (at 6.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 /F_VSYNC))
    (pad 34 smd rect (at 6.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 /F_DE))
    (pad 35 smd rect (at 7.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(P4-Pad35)"))
    (pad 36 smd rect (at 7.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 8.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /XP))
    (pad 38 smd rect (at 8.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 /YM))
    (pad 39 smd rect (at 9.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /XM))
    (pad 40 smd rect (at 9.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 /YP))
    (pad PD1 smd rect (at -11.9 -2.7 180) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad PD2 smd rect (at 11.9 -2.7 180) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5B0728D3)
    (at 93 95)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C6 (at 7.25 0 180) (layer F.SilkS))
    (fp_text value 33uF (at -0.09906 3.59918) (layer F.Fab) hide)
    (fp_text user + (at -5.48386 -2.26822) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeD_EIA-7343_HandSoldering (layer F.Cu) (tedit 5AFF43B5)
    (at 93 99.5)
    (descr "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (tags "Tantal Cap. , Size D, EIA-7343, Hand Soldering,")
    (attr smd)
    (fp_text reference C7 (at 7.5 0) (layer F.SilkS))
    (fp_text value 220uF (at -0.09906 3.59918) (layer F.Fab) hide)
    (fp_text user + (at -5.45846 -2.26822) (layer F.SilkS))
    (pad 2 smd rect (at 3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.88874 0) (size 4.0005 2.70002) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeD_EIA-7343_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:IDC_Header_Straight_10pins (layer F.Cu) (tedit 5B031A24)
    (at 89.5 80 90)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P2 (at 16 -4.5 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 5.08 5.223 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C1-Pad1)"))
  )
  (module AO_Parts:VQFN_48_7x7 (layer F.Cu) (tedit 5A54D866)
    (at 114 70 270)
    (attr smd)
    (fp_text reference U3 (at 5.5 0.25 360) (layer F.SilkS))
    (fp_text value FT810 (at 0 -5.08 270) (layer F.Fab) hide)
    (pad 43 smd oval (at -0.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 52 /R7))
    (pad 42 smd oval (at 0.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 /G2))
    (pad 41 smd oval (at 0.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 54 /G3))
    (pad 40 smd oval (at 1.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 /G4))
    (pad 39 smd oval (at 1.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 56 /G5))
    (pad 38 smd oval (at 2.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 57 /G6))
    (pad 37 smd oval (at 2.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 58 /G7))
    (pad 44 smd oval (at -0.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 51 /R6))
    (pad 45 smd oval (at -1.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 50 /R5))
    (pad 46 smd oval (at -1.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 49 /R4))
    (pad 47 smd oval (at -2.25 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 /R3))
    (pad 13 smd oval (at -2.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U3-Pad13)"))
    (pad 14 smd oval (at -2.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U3-Pad14)"))
    (pad 15 smd oval (at -1.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -1.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 17 smd oval (at -0.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 18 smd oval (at -0.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 19 smd oval (at 0.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 /XP))
    (pad 20 smd oval (at 0.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 /YP))
    (pad 21 smd oval (at 1.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 /XM))
    (pad 22 smd oval (at 1.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 /YM))
    (pad 23 smd oval (at 2.25 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd oval (at 2.75 3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-Pad24)"))
    (pad 6 smd oval (at -3.525 -0.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad10)"))
    (pad 5 smd oval (at -3.525 -0.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-Pad6)"))
    (pad 4 smd oval (at -3.525 -1.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R14-Pad1)"))
    (pad 3 smd oval (at -3.525 -1.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-Pad4)"))
    (pad 2 smd oval (at -3.525 -2.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd oval (at -3.525 -2.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R18-Pad2)"))
    (pad 7 smd oval (at -3.525 0.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-Pad7)"))
    (pad 8 smd oval (at -3.525 0.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U3-Pad8)"))
    (pad 9 smd oval (at -3.525 1.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd oval (at -3.525 1.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U3-Pad10)"))
    (pad 11 smd oval (at -3.525 2.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R12-Pad1)"))
    (pad 12 smd oval (at -3.525 2.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-Pad2)"))
    (pad 36 smd oval (at 3.525 -2.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 35 smd oval (at 3.525 -2.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /B2))
    (pad 34 smd oval (at 3.525 -1.725 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /B3))
    (pad 33 smd oval (at 3.525 -1.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /B4))
    (pad 32 smd oval (at 3.525 -0.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /B5))
    (pad 31 smd oval (at 3.525 -0.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /B6))
    (pad 30 smd oval (at 3.525 0.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /B7))
    (pad 29 smd oval (at 3.525 0.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /PCLK))
    (pad 28 smd oval (at 3.525 1.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 /DISP))
    (pad 27 smd oval (at 3.525 1.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 /HSYNC))
    (pad 26 smd oval (at 3.525 2.25 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /VSYNC))
    (pad 25 smd oval (at 3.525 2.75 270) (size 0.75 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 /DE))
    (pad 48 smd oval (at -2.75 -3.525 270) (size 0.25 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 /R2))
    (pad PD smd rect (at 0 0 270) (size 5.3 5.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AO_Parts:RPAK8 (layer F.Cu) (tedit 5A53E701)
    (at 119 81 270)
    (attr smd)
    (fp_text reference RN3 (at -3.5 0 360) (layer F.SilkS))
    (fp_text value "33 Ohms" (at 0 -1.8 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /B6))
    (pad 2 smd rect (at -1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /B7))
    (pad 3 smd rect (at -0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 /PCLK))
    (pad 4 smd rect (at -0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 /DISP))
    (pad 5 smd rect (at 0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 /HSYNC))
    (pad 6 smd rect (at 0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 /VSYNC))
    (pad 7 smd rect (at 1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 /DE))
    (pad 8 smd rect (at 1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RN3-Pad8)"))
    (pad 9 smd rect (at 1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(RN3-Pad9)"))
    (pad 10 smd rect (at 1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /F_DE))
    (pad 11 smd rect (at 0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /F_VSYNC))
    (pad 12 smd rect (at 0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /F_HSYNC))
    (pad 13 smd rect (at -0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /F_DISP))
    (pad 14 smd rect (at -0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /F_PCLK))
    (pad 15 smd rect (at -1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /F_B7))
    (pad 16 smd rect (at -1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /F_B6))
  )
  (module AO_Parts:RPAK8 (layer F.Cu) (tedit 5A53E638)
    (at 124.25 73 270)
    (attr smd)
    (fp_text reference RN2 (at -3.5 0 360) (layer F.SilkS))
    (fp_text value "33 Ohms" (at 0 -1.8 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /G4))
    (pad 2 smd rect (at -1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 /G5))
    (pad 3 smd rect (at -0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 /G6))
    (pad 4 smd rect (at -0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 /G7))
    (pad 5 smd rect (at 0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /B2))
    (pad 6 smd rect (at 0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /B3))
    (pad 7 smd rect (at 1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /B4))
    (pad 8 smd rect (at 1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /B5))
    (pad 9 smd rect (at 1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /F_B5))
    (pad 10 smd rect (at 1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /F_B4))
    (pad 11 smd rect (at 0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /F_B3))
    (pad 12 smd rect (at 0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /F_B2))
    (pad 13 smd rect (at -0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /F_G7))
    (pad 14 smd rect (at -0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /F_G6))
    (pad 15 smd rect (at -1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /F_G5))
    (pad 16 smd rect (at -1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /F_G4))
  )
  (module AO_Parts:RPAK8 (layer F.Cu) (tedit 5B073282)
    (at 126 65 270)
    (attr smd)
    (fp_text reference RN1 (at 3 -2.75 360) (layer F.SilkS))
    (fp_text value "33 Ohms" (at 0 -1.8 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /R2))
    (pad 2 smd rect (at -1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /R3))
    (pad 3 smd rect (at -0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /R4))
    (pad 4 smd rect (at -0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /R5))
    (pad 5 smd rect (at 0.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /R6))
    (pad 6 smd rect (at 0.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /R7))
    (pad 7 smd rect (at 1.25 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /G2))
    (pad 8 smd rect (at 1.75 0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /G3))
    (pad 9 smd rect (at 1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /F_G3))
    (pad 10 smd rect (at 1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /F_G2))
    (pad 11 smd rect (at 0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /F_R7))
    (pad 12 smd rect (at 0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /F_R6))
    (pad 13 smd rect (at -0.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /F_R5))
    (pad 14 smd rect (at -0.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /F_R4))
    (pad 15 smd rect (at -1.25 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /F_R3))
    (pad 16 smd rect (at -1.75 -0.65 270) (size 0.35 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /F_R2))
  )
  (module AO_Parts:CVS_1508 (layer F.Cu) (tedit 5A4FFA0D)
    (at 109 93)
    (fp_text reference LS1 (at 0 0) (layer F.SilkS))
    (fp_text value Speaker (at 4.2 -2) (layer F.Fab) hide)
    (fp_text user - (at -2.8 -3.8) (layer F.SilkS))
    (fp_text user + (at -2.8 3.6) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -3.8) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 104 "Net-(LS1-Pad1)"))
    (pad 2 thru_hole circle (at 0 3.8) (size 2 2) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 "Net-(LS1-Pad2)"))
  )
  (module AO_Parts:CPAK8 (layer F.Cu) (tedit 5B0D5C7C)
    (at 136.75 62.25)
    (attr smd)
    (fp_text reference CP1 (at -5.25 -1) (layer F.SilkS))
    (fp_text value "47 pF" (at 0 0.127) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /F_R5))
    (pad 2 smd rect (at -0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /F_R4))
    (pad 3 smd rect (at 0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /F_R3))
    (pad 4 smd rect (at 1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /F_R2))
    (pad 5 smd rect (at -1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /F_G2))
    (pad 6 smd rect (at -0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /F_G3))
    (pad 7 smd rect (at 0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /F_R7))
    (pad 8 smd rect (at 1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /F_R6))
    (pad 9 smd rect (at -3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AO_Parts:CPAK8 (layer F.Cu) (tedit 5B0D5C8A)
    (at 136.75 70.75)
    (attr smd)
    (fp_text reference CP2 (at -5.25 -1) (layer F.SilkS))
    (fp_text value "47 pF" (at 0 0.127) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 31 /F_G7))
    (pad 2 smd rect (at -0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /F_G6))
    (pad 3 smd rect (at 0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /F_G5))
    (pad 4 smd rect (at 1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /F_G4))
    (pad 5 smd rect (at -1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /F_B4))
    (pad 6 smd rect (at -0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /F_B5))
    (pad 7 smd rect (at 0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /F_B3))
    (pad 8 smd rect (at 1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /F_B2))
    (pad 9 smd rect (at -3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module AO_Parts:CPAK8 (layer F.Cu) (tedit 5B0D5C95)
    (at 136.75 79.25)
    (attr smd)
    (fp_text reference CP3 (at -5.5 -0.25) (layer F.SilkS))
    (fp_text value "47 pF" (at 0 0.127) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /F_DISP))
    (pad 2 smd rect (at -0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /F_PCLK))
    (pad 3 smd rect (at 0.635 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /F_B7))
    (pad 4 smd rect (at 1.905 -1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /F_B6))
    (pad 5 smd rect (at -1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /F_HSYNC))
    (pad 6 smd rect (at -0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 41 /F_VSYNC))
    (pad 7 smd rect (at 0.635 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 42 /F_DE))
    (pad 8 smd rect (at 1.905 1.524) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CP3-Pad8)"))
    (pad 9 smd rect (at -3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 3.175 0) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5B0859C7)
    (at 170 65.75 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value "MMBZ5250BLT 20V" (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822 180) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C18-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_MD-3030 (layer F.Cu) (tedit 5B08598B)
    (at 170 61.25 90)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-3030, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden md smd")
    (attr smd)
    (fp_text reference L1 (at 2.5 0 360) (layer F.SilkS))
    (fp_text value 22uH (at 0 3 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.1 0 90) (size 0.8 2.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_MD-3030.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A53DCAC)
    (at 179 61)
    (fp_text reference MH1 (at -5.5 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A53D782)
    (at 179 89)
    (fp_text reference MH2 (at -5.5 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A54D6CA)
    (at 78 61)
    (fp_text reference MH3 (at -5.5 -0.25) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5A53DDEB)
    (at 78 89)
    (fp_text reference MH4 (at -5.5 0) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5B085A0C)
    (at 173.75 61 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 3 0 360) (layer F.SilkS))
    (fp_text value BAT54 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B06E686)
    (at 82.5 59.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B081EDA)
    (at 106 69.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -3 -1 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B06C66C)
    (at 101.5 61 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 3 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B081431)
    (at 120.5 91.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 0.0047uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B086376)
    (at 106 70.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 1.5 -1.25 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A564C26)
    (at 125 91.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 0.0047uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0D5C25)
    (at 106 67.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -3 0.75 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A53EA2A)
    (at 129.25 91.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 0.0047uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A55415A)
    (at 132 88.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value "0.22 uF" (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B081D1D)
    (at 127.5 98.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0.75 -1.5 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0859F1)
    (at 165.75 65.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CF1)
    (at 99.75 86 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 -1.5 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B0819F2)
    (at 117 99 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at -1.25 -2.5 360) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06E6B9)
    (at 88.5 59.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(P1-Pad7)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06E663)
    (at 85.5 59.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(P1-Pad9)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B02E9F5)
    (at 84.5 88.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.5 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(P1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0334EA)
    (at 82.5 88.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.75 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(P1-Pad6)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06E66F)
    (at 84 59.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06C626)
    (at 99.5 61 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(P3-Pad9)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06C639)
    (at 97.5 61 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(P3-Pad10)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06C786)
    (at 88.5 88.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.5 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(P3-Pad8)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06E65B)
    (at 87 59.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(P1-Pad8)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06D063)
    (at 86.5 88.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3 0.5 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad5)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CCA)
    (at 104.25 76.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -3.25 450) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(P1-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B06F64B)
    (at 99 89.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(P1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CD0)
    (at 106 76.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -3 270) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(P1-Pad9)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CE9)
    (at 107.75 82.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -4 450) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CE2)
    (at 106 82.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -4.5 270) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(R15-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5CDC)
    (at 104.25 82.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -5 270) (layer F.SilkS))
    (fp_text value 33 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(P1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0732AD)
    (at 115.25 58.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -1.75 2.5 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B081391)
    (at 119.25 88.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(R18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B081395)
    (at 123.75 88.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 1.5 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0813C1)
    (at 128 88.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5C9E)
    (at 133 91.5 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 20k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B081493)
    (at 122.5 95.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -3.75 0) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(LS1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R21-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B085A30)
    (at 173 66 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 2.75 0 360) (layer F.SilkS))
    (fp_text value 1k (at -4 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(P4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A53D401)
    (at 195 75 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 4 0 90) (layer F.SilkS))
    (fp_text value 10 (at -4 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A53D406)
    (at 197 75 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 4 0 90) (layer F.SilkS))
    (fp_text value 10 (at -4 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SO-16-N (layer F.Cu) (tedit 5B072E3C)
    (at 108.5 61)
    (descr "Module CMS SOJ 16 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 7.25 2 180) (layer F.SilkS))
    (fp_text value 4050 (at 0 1.27) (layer F.Fab) hide)
    (pad 16 smd rect (at -4.445 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(R17-Pad1)"))
    (pad 13 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(R17-Pad1)"))
    (pad 10 smd rect (at 3.175 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at 4.445 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(R16-Pad1)"))
    (pad 8 smd rect (at 4.445 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.175 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(R15-Pad1)"))
    (pad 6 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R13-Pad1)"))
    (pad 4 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at -3.175 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -4.445 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 15 smd rect (at -3.175 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U1-Pad15)"))
    (model SMD_Packages.3dshapes/SO-16-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:TO-252-2Lead (layer F.Cu) (tedit 5B030046)
    (at 83 97 90)
    (descr "DPAK / TO-252 2-lead smd package")
    (tags "dpak TO-252")
    (attr smd)
    (fp_text reference U2 (at 4.25 -2.75 180) (layer F.SilkS))
    (fp_text value LM1117_3V3 (at 0 -2.413 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 -6.35 90) (size 6.096 6.096) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 2.286 0 90) (size 1.651 3.048) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/TO-252-2Lead.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AO_Parts:MSOP8 (layer F.Cu) (tedit 5B081468)
    (at 122.5 98 90)
    (attr smd)
    (fp_text reference U4 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value AP4991_MSOP (at 0 -3.6 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.975 2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-Pad7)"))
    (pad 2 smd rect (at -0.325 2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C14-Pad1)"))
    (pad 3 smd rect (at 0.325 2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(C14-Pad1)"))
    (pad 4 smd rect (at 0.975 2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(R21-Pad1)"))
    (pad 5 smd rect (at 0.975 -2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(LS1-Pad1)"))
    (pad 6 smd rect (at 0.325 -2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 7 smd rect (at -0.325 -2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -0.975 -2.105 90) (size 0.42 0.89) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(LS1-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B085ACF)
    (at 165.75 61.25 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at -2.5 2.25 360) (layer F.SilkS))
    (fp_text value LT1937 (at -0.05 2.35 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-Pad24)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5BE0)
    (at 166.5 71.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 1 1.5 180) (layer F.SilkS))
    (fp_text value 10k (at -4 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B085C55)
    (at 176 66)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 3.5 0) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B084139)
    (at 164.5 79.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 2.25 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5AFDF4C8)
    (at 93 61)
    (fp_text reference MH5 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5AFDF4DA)
    (at 194 61)
    (fp_text reference MH6 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5AFDF506)
    (at 93 89)
    (fp_text reference MH7 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:MH_M3x6mm (layer F.Cu) (tedit 5AFDF4F7)
    (at 194 89)
    (fp_text reference MH8 (at 0 4.25) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AO_Parts:FPC_40 (layer F.Cu) (tedit 5B059BDF)
    (at 183.25 78.5 180)
    (attr smd)
    (fp_text reference P5 (at -14 -6 180) (layer F.SilkS))
    (fp_text value FPC_40 (at 0 -3.5 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -9.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at -9.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(C18-Pad1)"))
    (pad 3 smd rect (at -8.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -8.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -7.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 6 smd rect (at -7.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 7 smd rect (at -6.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /F_R2))
    (pad 8 smd rect (at -6.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /F_R3))
    (pad 9 smd rect (at -5.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /F_R4))
    (pad 10 smd rect (at -5.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /F_R5))
    (pad 11 smd rect (at -4.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /F_R6))
    (pad 12 smd rect (at -4.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /F_R7))
    (pad 13 smd rect (at -3.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 14 smd rect (at -3.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 15 smd rect (at -2.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /F_G2))
    (pad 16 smd rect (at -2.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /F_G3))
    (pad 17 smd rect (at -1.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /F_G4))
    (pad 18 smd rect (at -1.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /F_G5))
    (pad 19 smd rect (at -0.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /F_G6))
    (pad 20 smd rect (at -0.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /F_G7))
    (pad 21 smd rect (at 0.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 22 smd rect (at 0.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (pad 23 smd rect (at 1.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /F_B2))
    (pad 24 smd rect (at 1.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /F_B3))
    (pad 25 smd rect (at 2.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /F_B4))
    (pad 26 smd rect (at 2.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /F_B5))
    (pad 27 smd rect (at 3.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 /F_B6))
    (pad 28 smd rect (at 3.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 /F_B7))
    (pad 29 smd rect (at 4.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at 4.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /F_PCLK))
    (pad 31 smd rect (at 5.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 /F_DISP))
    (pad 32 smd rect (at 5.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 /F_HSYNC))
    (pad 33 smd rect (at 6.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 /F_VSYNC))
    (pad 34 smd rect (at 6.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 /F_DE))
    (pad 35 smd rect (at 7.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(P5-Pad35)"))
    (pad 36 smd rect (at 7.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 8.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /XP))
    (pad 38 smd rect (at 8.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 /YM))
    (pad 39 smd rect (at 9.25 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /XM))
    (pad 40 smd rect (at 9.75 0 180) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 /YP))
    (pad PD1 smd rect (at -11.9 -2.7 180) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad PD2 smd rect (at 11.9 -2.7 180) (size 2.4 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B0D5BE6)
    (at 166.5 73.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at -1 1.75) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(P4-Pad14)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B083589)
    (at 172.25 71.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at -3.5 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B082B8B)
    (at 172.25 73.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 3.5 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(P4-Pad13)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B081EE4)
    (at 107.25 66 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:IDC_Header_Straight_10pins (layer F.Cu) (tedit 5B031A18)
    (at 100 80 90)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference P3 (at 16 -3.5 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 5.08 5.223 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P1-Pad9)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad5)"))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P1-Pad6)"))
    (pad 6 thru_hole oval (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P1-Pad8)"))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C1-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(P3-Pad9)"))
    (pad 10 thru_hole oval (at 10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(P3-Pad10)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B083CB1)
    (at 191.75 74.75 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5B0D5EDA)
    (at 186 61)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5B0D5EC9)
    (at 138 92)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module Fiducials:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 5B0D5F01)
    (at 123 77)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference REF** (at 3.4 0.7) (layer F.SilkS) hide)
    (fp_text value Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (at 0 -1.8) (layer F.Fab) hide)
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module AO_Parts:LulzBot_Logo (layer F.Cu) (tedit 0)
    (at 173 94)
    (attr smd)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 57FE9788)
    (at 187 67)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (target plus (at 73 56) (size 5) (width 0.1) (layer Edge.Cuts))
  (gr_text CLCD2 (at 145 93) (layer F.SilkS))
  (gr_line (start 73 102) (end 73 56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199 102) (end 73 102) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 199 56) (end 199 102) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73 56) (end 199 56) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "GNU GPLv3" (at 192 95) (layer F.SilkS))
  (gr_text "REV. A" (at 145 95) (layer F.SilkS))
  (gr_text "© 2018 Aleph Objects Inc.\nColor LCD User Interface" (at 144 99) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 198.5 101.5) (xy 73.5 101.5) (xy 73.5 56.5) (xy 198.5 56.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 198.5 101.5) (xy 73.5 101.5) (xy 73.5 56.5) (xy 198.5 56.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 198.5 101.5) (xy 73.5 101.5) (xy 73.5 56.5) (xy 198.5 56.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 198.5 101.5) (xy 73.5 101.5) (xy 73.5 56.5) (xy 198.5 56.5)
      )
    )
  )
)
